|  |
| --- |
| **Lockout/Tagout Program Audit Report** |
|  |  | **OK** | **Improvement Needed** |
| 1. | The written program is developed and accessible. | [ ]  | [ ]  |
| 2. | Awareness-level training is provided to affected employees.  | [ ]  | [ ]  |
| 3. | Full lockout/tagout training with lockout procedures for specific machinery and equipment is provided to authorized employees. | [ ]  | [ ]  |
| 4. | Skills evaluations are done as part of training. | [ ]  | [ ]  |
| 5. | Lockout/tagout supplies are readily available and good quality. | [ ]  | [ ]  |
| 6. | Locks are individually keyed. | [ ]  | [ ]  |
| 7. | Tags are readable and understandable, identify who is performing lockout, and contain instructions not to operate or energize equipment. | [ ]  | [ ]  |
| 8. | Lockout/tagout is performed for de-jamming activities. | [ ]  | [ ]  |
| 9. | Lockout/tagout is effective in that no employee can reach in or come into contact with areas where injury could occur. | [ ]  | [ ]  |
| 10. | The program addresses all applicable stored energies. | [ ]  | [ ]  |
| 11. | Specific lockout/tagout procedures are developed for each piece of machinery and posted on each piece of machinery.  | [ ]  | [ ]  |
| 12. | Lockout/tagout procedures are included for vehicles and mobile equipment. | [ ]  | [ ]  |
| 13. | Front-line supervisory staff observe employee behavior and enforce the lockout/tagout procedures. | [ ]  | [ ]  |
| 14. | Audits take place annually or more frequently. | [ ]  | [ ]  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** |  | **Audit by** |  |
| **Corrective Actions Needed** |
| **Actions and Responsible Persons** |
|  |